RELIABILT Aluminum Single Hung New Home Windows are designed for new construction and feature an integrated nail fin, making them very easy to install. These windows are energy-efficient and equipped with Low-E insulated glass that reflects heat from the sun during warm summer months while retaining warmth inside during colder winter months. RELIABILT aluminum single-hung windows are manufactured from an extruded aluminum sash and main frame that is durable and maintenance-free and includes an easily removable screen that keeps insects out. RELIABILT Aluminum Single Hung Windows complement any surroundings, require no painting, and are backed by a lifetime manufacturer's warranty.

* Designed for new construction, the RELIABILT 46000 series single-hung home windows feature low-E double-pane glass to provide a cost-effective window with unbeatable performance
* Low-E insulated glass on exterior windows reduces condensation and improves thermal energy efficiency by reflecting the sun's heat away from your home during the warm summer months, and helps keep warmth inside in colder winter months
* Aluminum bottom sash interlocks with the main frame for added strength, durability, and security, ensuring a weather-tight seal on these new windows
* White exterior and white interior extruded aluminum main frame is maintenance-free and durable for long-lasting performance
* Windows open and close smoothly thanks to the block-and-tackle balance system, then lock securely into place with 2 sweep locks to seal gaps and prevent drafts
* Internal weeping system prevents moisture buildup, and a removable half screen keeps unwanted insects out
* Low maintenance aluminum finish never needs painting, and complements any surroundings
* Installation is easy, especially with the integrated nail fin for a secure and stable installation
* Backed by a limited lifetime manufacturer warranty

| **General** | | | |
| --- | --- | --- | --- |
| **Color/Finish Family** | White | **Interior Color/Finish** | White |
| **Exterior Color/Finish** | White | **Series Name** | 46000 Series |
| **Hardware Color/Finish** | White |  |  |
|  |  |  |  |
|  |  |  |  |

| **Dimensions** | | | |
| --- | --- | --- | --- |
| **Actual Size (W x H)** | 35-1/2-in x 47-1/2-in | **Jamb Depth Measurement** | 2-5/8-in |
| **Clear Opening Size (W x H)** | 33-3/4-in x 18-in | **Rough Opening Size (W x H)** | 36-in x 48-in |
| **Common Size (W x H)** | 36-in x 48-in | **Weight (lbs.)** | 42 |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

| **Features** | | | |
| --- | --- | --- | --- |
| **Argon Gas Insulated** | No | **Insect Screen Included** | Yes |
| **Balance System** | Block and tackle | **Lock Type** | Sweep |
| **Clear Opening Sq Ft** | 4.22 | **Lowe's Exclusive** | Yes |
| **Design Pressure (DP) Rating** | 40 | **Nail Fin** | Integrated |
| **For Use with Mobile Homes** | Yes | **Number of Locks** | 2 |
| **Frame Material** | Aluminum | **Obscure Glass** | No |
| **Frame Profile** | Flat | **Paintable** | No |
| **Glass Insulation** | Low-E | **Project Type** | New construction |
| **Glass Strength** | Single strength | **Screen Frame Type** | Roll-form |
| **Glazing Type** | Double pane | **Screen Included** | Half |
| **Grid Included** | No | **Screen Type** | Fiberglass mesh |
| **Grid Pattern** | None | **Solar Heat Gain Coefficient (SHGC)** | 0.33 |
| **High Altitude Rated** | No | **Tilting** | No |
| **Impact Resistant** | No | **Wood Jamb Extension** | None |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

| **Certifications** | | | |
| --- | --- | --- | --- |
| **CA Residents: Prop 65 Warning(s)** | No | **Meets CA Forced Entry Requirements** | No |
| **ENERGY STAR Certified North/Central Zone** | No | **Meets Title 24** | No |
| **ENERGY STAR Certified Northern Zone** | No | **Meets Wildland Urban Interface** | No |
| **ENERGY STAR Certified South/Central Zone** | No | **Miami Dade Approved** | No |
| **ENERGY STAR Certified Southern Zone** | No | **Sound Transmission Control (STC) Rated** | No |
| **Florida Product Approved** | No | **Texas Department of Insurance Approved** | No |
| **Hurricane Approved** | No | **U Value** | 0.52 |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

| **Warranty** | | | |
| --- | --- | --- | --- |
| **Warranty** | Limited lifetime |  |  |

| **Miscellaneous** | | | |
| --- | --- | --- | --- |
| **UNSPSC** | 30171600 |  |  |